| **Items** | **Remarks** | **1st Use Check** | **New Genset Every 50**  **Hour** | **Every 100**  **Hour** | **Every 200**  **Hour** | **Every 400**  **Hour** | **Every 1000**  **Hour** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Oil | Check Oil Level | ● |  |  |  |  |  |
| Replace |  | ● | ● |  |  |  |
| Oil Filter | Replace |  | ● |  | ● |  |  |
| Air Filter | Clean |  |  | ● |  |  |  |
| Replace Filter Element |  |  |  |  | ● |  |
| Spark Plug | Check |  |  | ● |  |  |  |
| Replace |  |  |  |  | ● |  |
| Cooling System | Check Coolant Level and Leakage Occurs | ● | ● | ● |  |  |  |
| Clean radiator |  |  |  | ● |  |  |
| Check the fan running condition |  |  |  | ● |  |  |
| Check radiator hose connection |  | ● |  | ● |  |  |
| Change the coolant |  |  |  |  | ● |  |
| Gas Valve | Check/adjust | ● |  |  | ● |  |  |
| Gas Pipe | Check the gas pipe is damage or not |  | ● |  |  | ● |  |
| Exhaust System | Check to see if there is leakage, tighten or replace if needed |  | ● |  |  |  | ● |
| Screw and  Nut | Check all screws, nuts whether become loosen and then screw down. |  | ● |  | ● |  |  |
| Water Pump Belt | Adjust tension |  | ● | ● |  |  |  |
| Replace |  |  |  |  |  | ● |
| Aging Wires | Check all wires for aging situation and if the connectors are loose or not |  | ● |  | ● |  |  |
| Timing Belt | Depends on the wear pattern | Change Every 1200 Hours | | | | | |